1. THERMOPLASTIC TREATMENT [620] (Revised 8-16-11)

Description. This work is the preparation of existing thermoplastic pavement markings prior to the seal coat application.

Construction. Mechanically scarify and roughen existing thermoplastic pavement marking surfaces to produce a uniformly roughened surface that, when sealed, is smooth and matches adjacent surfaces.

Method of Measurement. Thermoplastic treatment is measured as a lump sum.

Basis of Payment. Payment for the completed and accepted quantities is made under the following:

|  |  |
| --- | --- |
| Pay Item | Pay Unit |
| Thermoplastic Treatment | Lump Sum |

Payment at the contract unit price is full compensation for all resources necessary to complete the item of work under the contract.