1. STRUCTURE EXCAVATION – COFFERDAMS (Revised 5-29-03)

Description. Excavation for any substructure unit located within the active streambed as defined in the Special Provision titled Cofferdams is restricted to the area within an approved cofferdam.

Construction Requirements. Transport and stockpile material excavated during substructure construction for future use in backfilling the excavation. Locate the stockpiles so that sediment and silt laden water does not drain back into the stream or adjacent wet lands. Handle all excavated material in a manner that prevents adding turbidity to the stream.

Basis of Payment. Payment for all costs associated with excavating, handling, transporting, stockpiling and backfilling is included in the unit price bid for Structure Excavation, Type II.