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	SPECIAL PROVISIONS




glass beads [714] (added 10-22-26)
Roundness for glass spheres must have a minimum of 80% true spheres in accordance with AASHTO M247 for Contracts LET on or after January 14, 2027. 
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